Skip to main content

## Tips & Tricks

Some tips around Lisp files

If developers would like to provide one installation for both AutoCAD and BricsCAD, encrypted Lisp files should use standard *.des filename extension - this ensures, that AutoCAD will load the normal *.fas/*.vlx files, and BricsCAD will load *.des files.

For this scenario, developers should always use the (load "name") function syntax, excluding the filename extension - BricsCAD uses the following searching order :

1. <filename>.des

2. <filename>.lsp

3. <filename>.prt (for protected lisp files, generated by Protect.exe)

4. <filename>.klv (Kelvinated lisp files)

This searching order ensures that encrypted Lisp files *.des are primarily used under BricsCAD (if present) - thus, preventing conflicts with existing fas/vlx files (if also present). With this design we hope to offer most compatible Lisp loading technology together with smallest impact to Lisp developers.

####