Skip to main content

## MLEdit

Edit MultiLine vertices, cuts / breaks, and intersections

| Command: MLEdit

This command opens the MultiLine Edit dialog.

| There are several utilities provided to modify multiline crossings, connections and vertex sequence. Due to missing API support in DwgDirect and BricsCAD, most of these functions are not yet available - but we are working on it to get some of the more important functions to be implemented in near future. We are very sorry for this inconvenience !

| Closed Cross creates a "closed cross" intersection from 2 selected multilines - the first selected multiline has priority.

| Open Cross creates an "open cross" intersection from 2 selected multilines - for the second multiline, only the outer-most lines will get breaks.

| Merged creates an "merged cross" intersection from 2 selected multilines - both multilines have same priority.

| Closed Tee creates a "closed tee" intersection - the first multiline is trimmed resp. extended to the second multiline.

| Open Tee creates an "open tee" intersection - the first multiline is trimmed resp. extended to the second multiline, which is also opened.

| Merged Tee creates a "merged tee" intersection - the first multiline is trimmed resp. extended to the second multiline.

| Corner Joint creates a "corner joint" intersection - the elements of both multilines are trimmed resp. extended to their intersections.

| Add Vertex inserts a new vertex into the multiline.

| Remove Vertex removes a vertex from the multiline.

| Cut Single inserts a cut into selected element of a multiline.

| Cut All inserts a cut into all elements of a multiline.

| Weld All removes all cuts from all multiline segments.

####